Column            Parameter
1      Start Time as YYYY-MM-DDTHH:MM:SS.dddZ where T is for Time and Z for Zulu
2      End Time as YYYY-MM-DDTHH:MM:SS.dddZ where T is for Time and Z for Zulu
3      Spacecraft as C# where C stands for Cluster and # for number
4      Conversion Frequency (0, 125, 250 or 500)
5      Units for Conversion Frequency (kHz)
6      Bandwidth Frequency Extent (9.5, 19 or 77)
7      Units for Bandwidth Frequency Extent (kHz)
8      Antenna (Ey, Ez, By or Bz)
9      Resolution (1, 4 or 8)
10     Units for Resolution (bits)
11     Data or Acquisition Type:
       B:  Burst Mode-2 continuous digitally filtered data, 1/3 sampling rate -- same as BF3
       BDC:  Burst Mode-2 duty cycled (keep 1 out of every 3 frames) -- same as BDC3
       BDC3: Burst Mode-2 duty cycled (Keep 1 out of every 3 frames)
       BDC4: Burst Mode-2 duty cycled (Keep 1 out of every 4 frames)
       BF:  Burst Mode-2 continuous digitally filtered data, 1/3 sampling rate -- same BF3
       BF3:  Burst Mode-2 continuous digitally filtered data, 1/3 sampling rate
       BF4:  Burst Mode-2 continuous digitally filtered data, 1/4 sampling rate
       PAN: TDA8 real time data received at Panska Ves
       If none of the types listed above are
       shown, data is TDA8 from either DSN or Panska Ves.
