MAG STATUS Word Definitions


Bit 1 is on the left (MSB) and bit 16 is at the right (LSB)

Bit
1  2  3  4  5  6  7  8  9 10 11 12 13 14 15 16
MSB                                        LSB


MAG STATUS WORD 1 (STAT1)

Bit 1     OBLFM range mode 
          0 = manual
          1 = auto

Bit 2     OBLFM range bit 1 (LSB)

Bit 3     OBLFM range bit 2

Bit 4     OBLFM range bit (MSB)

Bit 5     IBLFM range mode 
          0 = manual
          1 = auto

Bit 6     IBLFM range bit 1 (LSB)

Bit 7     IBLFM range bit 2

Bit 8     IBLFM range bit 3 (MSB)

Bit 9     OBHFM range mode 
          0 = manual
          1 = auto

Bit 10    OBHFM range bit 1
          0 = low
          1 = high

Bit 11    IBHFM range mode 
          0 = manual
          1 = auto

Bit 12    IBHFM range bit 1
          0 = low
          1 = high

Bits 13,14,15,16  Fill bits

-------------------------------------------------------




MAG STATUS WORD 2 (STAT2)

Bit 1     OBLFM in flight calibration
          0 = OFF
          1 = ON

Bit 2     IBLFM in flight calibration
          0 = OFF
          1 = ON

Bit 3     OBHFM in flight calibration
          0 = OFF
          1 = ON

Bit 4     IBHFM in flight calibration
          0 = OFF
          1 = ON

Bit 5     IFC polarity
          0 = negative
          1 = positive

Bit 6     Processor selection
          0 = processor A selected
          1 = processor B selected

Bit 7     IBLFM flipper
          0 = 0
          1 = 180

Bit 8     IBLFM flipper
          0 = locked
          1 = unlocked

Bit 9     OBLFM flipper
          0 = 0
          1 = 180

Bit 10    OBLFM flipper
          0 = locked
          1 = unlocked

Bit 11    Prime LFM status
          0 = outboard prime
          1 = inboard prime

Bit 12    Electrical flipper
          0 = normal
          1 = reversed

Bits 13,14,15,16  Fill bits

